{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Tabelle1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Tabelle1","index":0,"n_rows":20,"n_cols":7,"rows_kept":20,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[null,null,"Lunghezza della corsa","Hublänge","Stroke length",35,"mm"]
[null,null,"Velocità di rotazione della torretta","Drehzahl Revolverkopf","Rotational speed turret",{"$f":"IF((F6*1000)/(F4*2)>750,\"Drehzahl zu hoch\",(F6*1000)/(F4*2))","v":742.85714285714289},"U/min"]
[null,null,"Velocità di taglio / Materiale","Schnittgeschwindigkeit / Material","Cutting speed / Material",52,"M/min"]
[null,null,"Avanzamento in profondità in X per corsa dello slittamento","Tiefenzuführung in X pro Hub","Depth feed in X per slide stroke",0.02,"mm"]
[null,null,"Profondità della scanalatura","Nuttiefe","Depth of groove",1.9,"mm"]
[null,null,"Corsa","Hübe","Strokes",{"$f":"(F8/F7)","v":95}]
[null,null,"Profondità della scanalatura / Avanzamento x Lunghezza della scanalatura","Nuttiefe / Zuführung x Nutlänge","Depth of groove / Feed x Length of groove",{"$f":"(F8/F7)*F4","v":3325},"mm"]
[null,null,"Tempo di lavorazione per scanalatura in ","Bearbeitungszeit pro Nut in ","Processing time per groove in ",{"$f":"F10/F15","v":6.3942307692307687E-2},"Min"]
[null,null,"Tempo di lavorazione per scanalatura in ","Bearbeitungszeit pro Nut in ","Processing time per groove in ",{"$f":"F11*60","v":3.8365384615384612},"Sec"]
[null,null,"Numero di forme","Anzahl Nuten","Number of forms",21,"pc"]
[null,null,"Tempo totale di lavorazione ","Gesamtbearbeitungszeit ","Total processing time ",{"$f":"F12*F13","v":80.567307692307679},"sec"]
[null,null,"Distanza/min","Strecke/min","Distance/min",{"$f":"(F6*1000)","v":52000},"mm"]
[null,null,"Corsa","Verfahrweg","Travel",{"$f":"F5*(F4*2)","v":52000},"mm"]
[]
[{"$nulls":4},"Data entry only in the fields highlighted in yellow"]
[]
[{"$nulls":4},"Material in this case:","31CrMoV9"]